A

A

1 1

1 uS Pulse width = 6.5*Tclk

EIA 422

TYPICAL TRIGGER CHANNEL, 30 TOTAL

SCSI 68 PIN CONNECT OR

P4 & P5 SCSI 68 PIN CONNEC TORS

P2 50 PIN BACKPLANE CONN.

P1 96 PIN HPIB BACKPLANE CONN.

Time Stamp Enable FF

TRIGGER CONDITONER BOARD C 7-99 -

U C S B H E P

Santa Barbara, CA

CDMS 2 A 1 1 Tuesday, July 27, 1999

Size Document Number Rev

Date: Sheet of

VCC

D CLK Q

R Q

D CLK Q

R Q

D CLK Q

R Q

100K

D CLK Q

R Q

D CLK Q S

RTF TRIG IN

WRITE

TRIGGER OUT

TIME STAMP + DIN

PWR-UP

TIME STAMP -

6.5 Mhz

DOUT